**LED PANEL ORDER FORM**

|  |
| --- |
| **Order Information** |
| Project/Customer: |  |  |
|  |
| **Luminaire Information** |
| Article: |  |  |
| Type: |  |  |
| Quantity: |  |  |
| CRI: |  |  |
| CCT: |  |  |
| Power: |  |  |
| Size: |  |  |
| Dimming: |    |  |  |  |
| Luminous flux: |  | lm |
| Warranty: |  | years |
|  |
| **Cable Accessories**A – assembled with luminaire; B – supplied separately  |
| Connection cable 2x1.5mm2 (x2.5m) with open end |  |  |  |  |  |
| Connection cable 5x1.5mm2 (x2.5m) with open end |  |  |  |  |  |
| Connection cable 3x1.5mm2 (x2.5m) with plug |  |  |  |  |  |
| Connection cable with DALI 5x1.5mm² (x2.5m) with WAGO Winsta (770-1115) 5-way plug |  |  |  |  |  |
| Connection cable 2x1.5mm2 (x2.5m) with WAGO Winsta (770-112/041-000) 2-way plug |  |  |  |  |  |
| Connection cable 2x1.5mm2 (x2.5m) with Ensto (NAC21S.W) 2-way plug |  |  |  |  |  |
| Connection cable 5x1.5mm2 (x2.5m) with Ensto (NAC51S.W) 5-way plug |  |  |  |  |  |
| Other |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **Accessories**A – assembled with luminaire; B – supplied separately  |
| Microwave sensor |  |  |  |  |  |
| Gypsum Board mounted frame / for 600\*600mm |  |  |  |  |  |
| Push-in Surface mounted frame / For 600\*600mm |  |  |  |  |  |
| Decorative plate |  |  |  |  |  |
| Suspension kit / 4 pcs suspension cable 1000mm |  |  |  |  |  |

|  |
| --- |
| **Other Requirements** |